Bell 205A1++ Helicopter Specifications

**\*\*NOTE: If vendors choose to not comply with certain specifications listed. Those exceptions must be identified and documented on a separate sheet and uploaded as part of the vendors response.**

To provide a Bell 205A1++ Helicopter with required the following required equipment:

**Vendor Complies \_\_\_\_\_ YES \_\_\_\_\_ NO**

* Dual Controls
* Bleed Air Heater
* Wire Strike Protection
* High Skid Gear with Flight Steps
* BLR Strake and Fast Fin
* Donaldson Inlet Barrier Filter
* Dart L/H Pilot in command kit
* Standard L/H Vertical Reference Door
* Dart Cabin Door Roller kit
* Cargo Hook with Load Cell
* Cargo Mirrors with Pulselight
* Dart Co-Pilot External Hook Release
* AEM (ex-Eagle) Digital Audio Panel with two aft transmit stations
* Garmin GTN750Xi GPS/NAV/Com/MFD
* Garmin GTN650 GPS/NAV/Com/MFD
* Garmin GTX 345R Transponder
* Garmin GTS 825 TAS System
* Garmin GRA 55 Rad-Alt with Dual GI205
* Sirius XM Weather with music
* Dual Technisonic TDFM 136NV FM Radios
* NVIS Compatible Flight Deck
* External Rescue Hoist Goodrich
* Fresh exterior Paint to customer specifications

**COMPONENTS:  
Vendor Complies \_\_\_\_\_ YES \_\_\_\_\_ NO**

1. Proposed Helicopter delivered with no less than 1000 hours or 50% of service life remaining on components and accessories.
2. Exceptions to above the following will be Overhauled or NEW:
3. M/R Blades NEW
4. Tail Rotor Blades NEW
5. M/R Hub Overhauled, with Yoke NEW.
6. M/R Transmission Overhauled.