JOHN DEERE 544 P-TIER WHEEL LOADER W/KODIAK 3036 SNOW BLOWER

SPECIFICATIONS

**\*\*NOTE: If vendors choose to not comply with certain specifications listed. Those exceptions must be identified and documented on a separate sheet and uploaded as part of the vendors response.**

To provide a John Deere 544 P-Tier Wheel Loader W/Kodiak 3036 Snow Blower with the following standard equipment:

**Vendor Complies \_\_\_\_\_ YES \_\_\_\_\_ NO**

* JDLink
* United States
* English
* Translated Text Labels
* Standard Loader
* Standard Z-Bar
* Level 2 Trim
* Level 1 Performance
* Rear Camera (Primary Display)
* Less Detection System
* Left Side Steps
* Less Payload Scale w/Cycle Counter
* John Deere 6.8L – FT4/SV
* Bridgestone VJT – 20.5R25 L3 1-Star Radial Tires w/3 PC Rims
* Full Coverage Front Fenders
* Rear Counterweight and Rear Hitch w/Pin
* Joystick Controls
* Three Function Hydraulics
* Hydraulic Coupler – JRB 416 Patter
* Bolt-On Cutting Edge
* 3.00 YD (2.30 CM) Enhanced Performance
* Heated and Powered Exterior Mirrors
* Maintenance and Service Package
* Guards – Transmission & Bottom
* Two (2) sets of tire chains
* Kodiak LMSC3036 Snow Blower
* Extended Warranty