**80DOT-S2522**

**COMPACT TRACK LOADER SPECIFICATIONS**

**\*\*NOTE:  If vendors choose to not comply with certain specifications listed.  Those exceptions must be identified and documented on a separate sheet and uploaded as part of the vendors response.**

**Machine Specifications**

279D3 Compact Track Loader

Lane 2 Order

Pack, Domestic Truck

Shipping/Storage Protection

Heater, Engine, Coolant, 120V

Counterweight, Machine, External

Rear Lights

Track, Rubber, 450MM (17.7IN) Black

Oil, Hydraulic, Cold Operation

Serialized Technical Media Kit

Film, Ride Control, ANSI

Instructions, ANSI, USA

Door, Cab, Glass

Seat Belt, 3”

Ride Control

Certification Arr, P65

Product Link, Cellular PL641

Battery, Extra Heavy Duty, Disc

Cab Package, Ultra

Hydraulics, Performance, (H3)

Control, ISO, Prop, Wt

Lights, LED

Rubber Belt, 2 spd, TF Idlers

ROPS, Enclosed with A/C (C3)

Display, Advanced, LCD, Camera

Fan, Cooling, Demand

Quick Coupler, Hydraulic

Sea, Air Suspension, Cloth, Heat

Film, Two Speed w/ High Flow XPS

Standard Radio (12V), Bluetooth

Bucket-GP, 80”, BOCE

Warranty & Coverage, Standard Warranty, 24 month/2000 hours which include travel time and mileage for first twelve months.

**Vendor complies with all specifications listed above: YES\_\_\_\_\_\_\_\_\_\_ NO\_\_\_\_\_\_\_\_\_\_**