**80DOT-S2526**

**2023 CAT MODEL 309-07 EXCAVATOR**

**\*\*NOTE:  If vendors choose to not comply with certain specifications listed.  Those exceptions must be identified and documented on a separate sheet and uploaded as part of the vendors response.**

**Machine Specifications**

309 07A CR MHE DCA16D

309 07A CR MINI EXCAVATOR

DRAIN, ECOLOGY

HEATER, WATER JACKET

SEAT, AIR SUSP, FABRIC, HEATED

BELT, SEAT, 3” RETRACTABLE

ALARM, TRAVEL

MONITOR NEXT GEN, ADVANCED, CR

LIGHTS, LED

INTEGRATED RADIO

CAMERA, REAR VIEW

ELECTRICAL ARR, C3.3 HRC

BOOM, SWING

LINES, BOOM

LINES, STICK

LINES, QC, LNG STK, 3 LINE

ENGINE, EPA TIER 4 FINAL

CONTROL, QC, 3 LINE

CAT KEY, WITH PASSCODE OPTION

INSTRUCTIONS, ANSI

INSTRUCTIONS, CANADA

COUNTERWEIGHT, EXTRA

FILM, COUPLER, ISO

SOFTWARE, PROPORTIONAL CONTROL

SOFTWARE, STICK STEER CONTROL

SOFTWARE, 2 WAY CONTROL

SOFTWARE, CODED START

PRODUCT LINK, CELLULAR PLE643

STOCK, LONG, HIGH FLOW

STD BLADE, LONG U/C TG W/PAD

LINKAGE, BUCKET W/ LIFTING EYE

EOU HOUSE SWING COVER, 8T

WIRING GP

COVER GP

PLUG GP

SHIPPING/STORAGE PROTECTION

PACKING, LAST MILE PROGRAM

SERIALIZED TECHNICAL MEDIA KIT

LANE 2 ORDER

COUPLER, PG, HYRO.D.LOCK, 7-9T

BUCKET HD, 24”

Warranty & Coverage, Standard Warranty, 24 month/2000 hours which include travel time and mileage for first twelve months.

**Vendor complies with all specifications listed above: YES\_\_\_\_\_\_\_\_\_\_ NO\_\_\_\_\_\_\_\_\_\_**